Rate Current(A),42.9
Max Current Percent(%),200
Rotor Innertia(kgcm2),7900
Rate Torque(NM),150
Stator Register(om),0.32
Rotor Register(om),0.3
Total Leak Induct(mL),1.4
Lm Induct(mL),150
Rate Freq(Hz),50
Max Freq(Hz),100
Pair of Poles,2
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,1
Default current loop bandwidth,1000
Default speed loop bandwidth,10
Default encoder filter ,5
Default encoder sample period setting ,2
Others Parameter Set:

