40-Cam engagement output
41-Sync area output
42-close to output of Order 
43-Order Completion Output
51-Color mark trigger valid range output
52-Output the signal that the current set cutting length is too small
53-hardware limit output
54-Software limit output
55-Special-purpose servo zero return complete output
56-Stop output
