Rate Current(A),103.6
Max Current Percent(%),200
Rotor Innertia(kgcm2),5362
Rate Torque(NM),350
Stator Register(om),0.32
Rotor Register(om),0.3
Total Leak Induct(mL),1.4
Lm Induct(mL),150
Rate Freq(Hz),50
Max Freq(Hz),150
Pair of Poles,2
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Default current loop bandwidth,300
Default speed loop bandwidth,20
Default encoder filter ,5
Default encoder sample period setting ,2
Others Parameter Set:

