Rate Current(A),2.8
Max Current Percent(%),250
Rate Speed(rpm),3000
Max Speed(rpm),6000
Rotor Innertia(kgcm2),0.39
Rate Torque(NM),1.27
EMF(V/Krpm),0
Stator Register(om),3.04
Stator Induct(mL),9.34
Electric Time Constant(ms),3
Pair of Poles,4
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Z point offset,2473
HALL1 electric angle,442
HALL2 electric angle,94
HALL3 electric angle,264
HALL4 electric angle,774
HALL5 electric angle,609
HALL6 electric angle,947
Default current loop bandwidth,2035
Default speed loop bandwidth,35
Default encoder filter ,5,0
Default encoder sample period setting ,0
Others Parameter Set:

