66-Sampling length， the next cycle runs according to the immediate cutting length， and the rising edge is valid
68-In point cam mode， switch to auxiliary color mark. if this function but is valid， use auxiliary color code
69-In point cam mode， auxiliary colour mark.
70-The tangent point is confirmed， and the rising edge is valid. For specific usage， please refer to 5.18.
71-The spindle position source is switched.
72-Cam meshing is enabled， effective when the effective level is high， meshing when it is effective， and disengaging when it is ineffective.
73-CAM pause signal， effective when the effective level is high.
74-The origin returns to zero，
75-Colour mark signal input， this function is DI9 of fixed driver.
76-Origin signal input， this function is DI10 of fixed driver .
77-Colour mark manual shielding input， effective when the effective level is high， colour mark trigger is invalid when effective
78-Feeding detection signal， effective when the effective level is high
79-Cut the signal immediately， the rising edge is valid
80-Trigger an interrupt event， the rising edge is valid
81-Switch from the interrupt event to the cam mode， the cam re-engages， and the rising edge is valid
82-Clear the number of effective switching points P16.07， effective when the effective level is high
83-Clear the total number of cuts P16.08， order 1 count P15.91， order 2 count P15.92， order 3 count P15.93， order 4 count P15.94， valid when the effective level is high
84-Clear the colour mark count P16.35， valid when the effective level is high
85-The current order count is cleared， valid when the effective level is high
86-The wheel tangent is jog in the positive direction， it can only be used when it is disengaged， and it is effective when the effective level is high.
87-The wheel tangent is jog in the reverse direction， it can only be used when it is disengaged， and it is effective when the effective level is high.
88-Spindle positive jog phase shift， effective when the effective level is high
89-Spindle reverse jog phase shift， effective when the effective level is high
90-pull gauge signal 
91-single signal 
92-double sheet signal 
93-Increase the distance from the pull gauge to the tangent point 
94-Reduce the distance from the pull gauge to the tangent point 
95-Relearn the distance from the pull gauge to the tangent point
96-Enable servo and enable cam
97-Switch between fixed-length cutting mode or color mark tracking mode
98-Clear wheel tangent alarm