40-Output signal (position reached )
41-Output signal (pressure reaches )
42-Output signal (return to zero point)
43-Output signal (excessive pressure)
45-Output signal (hardware limit position)
46-Output signal (software limit position)
47-Output signal (return to safe position)
48-Output signal (superposition position reached)
50-Output signal (pressing)
51-Output signal (press-fitting)
52-Output signal (returning)
55-Output signal ((speed command module) is running)
56-Output signal ((speed command module) has reached the set speed)
57-Output signal ((stop command module) is running)
58-Output signal ((stop command module) stop reaching, lock position)
59-Output signal ((Position command module) is running)
60-Output signal ((position command module) reaches the set position), at this time OUTFn.59 is invalid
61-Output signal ((Position superposition instruction module) is running)
62-Output signal ((position superposition command module) has reached the set position), at this time OUTFn.61 is invalid
63-Output signal ((PID (pressure holding) command module) is running)
64-Output signal ((PID (pressure holding) command module) reaches the set position), the press fitting has not touched the product
65-Output signal ((PID (pressure holding) command module) is in contact with the product)
66-Output signal ((PID (pressure holding) command module) current pressure reaches target value)
67-Output signal (zero return command module) is running)
68-Output signal (zero return command module) zero return complete)
