68 - Cut complete
69-Forward jog fixed position (tension type: motor rotation direction in closed-loop speed mode) (second color code of point cam)
70 - Pointcut Confirm DI
71-Cam spindle position source XY pulse and the second encoder switching
72-Enable the CAM
73 - Pause Cam Input
74 - zero return input bit
75-Mark color mark signal input, fixed servo driver DI9
76-Origin signal signal input, fixed servo driver DI10
77- Color mark shielding 
78-Feeding detection signal， effective when the effective level is high
79-Cut the signal immediately， the rising edge is valid
80-Trigger an interrupt event， the rising edge is valid
81-Clear the current cycle color mark count
82 - Clear cut count
83-Clear the total number of cuts
84-Color mark count is cleared
85-The current order count is reset to zero
86-Slave axis forward jog
87-Slave axis reverse jog
88-Spindle forward jog phase shift
89-Spindle reverse jog phase shift
90-Online cut length correction, data save when power off
91-Online cut length correction, data is not saved when power off
47-Order switch 1, valid when the valid level is high
48-Order switch 2, valid when the valid level is high
49- Positive phase shift of the spindle, every time it is triggered, the spindle will increase the displacement of P16.44
50-Spindle negative phase shift, every time it is triggered, the spindle reduces the displacement of P16.44
51-Increase the cutting length of the current order, each time it is triggered, the cutting length of the current order increases by P15.37
52- Decrease the cutting length of the current order, every time it is triggered, the cutting length of the current order is reduced by P15.37
