Rate Current(A),5.5
Max Current Percent(%),249
Rate Speed(rpm),1500
Max Speed(rpm),3000
Rotor Innertia(kgcm2),36.2
Rate Torque(NM),17
EMF(V/Krpm),0
Stator Register(om),3.94
Stator Induct(mL),11.5
Electric Time Constant(ms),2
Pair of Poles,4
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Z point offset,2473
HALL1 electric angle,455
HALL2 electric angle,109
HALL3 electric angle,273
HALL4 electric angle,801
HALL5 electric angle,631
HALL6 electric angle,967
Default current loop bandwidth,1681
Default speed loop bandwidth,11
Default encoder filter ,5,0
Default encoder sample period setting ,0
Others Parameter Set:

