171-Spindle position source switching， when it is valid， it comes from the second encoder， and when it is invalid， it comes from XY pulse. Fixed drive DI6.
172-Cam engagement is enabled， valid when the valid level is high，engages when valid， disengages when invalid
173-Cam pause signal， valid when the valid level is high
174-The origin returns to zero， the rising edge is valid
175-Color mark signal input， fixed driver DI9.
176-Origin signal input， fixed driver DI10.
177-Color mark manual shielding input， valid when the valid level is high
178-Feed detection signal， valid when the active level is high
179-Cut the signal immediately， the rising edge is valid
180-Trigger the interrupt event， the rising edge is valid
181-Switch from interrupt event to cam mode， cam re-engages， rising edge valid
182-Clear the number of valid cut points P16.07， valid when the valid level is high
183-The number of times of clearing P16.08， P15.91， P15.92， P15.93 and P15.94， valid when the valid level is high
184-Clear the color mark count P16.35， valid when the active level is high
185-The current order count is cleared， valid when the valid level is high
186-Wheel cut forward jog， valid when the valid level is high
187-Wheel cut reverse jog， valid when the valid level is high
188-Spindle Forward jog phase shift， valid when the valid level is high
189-Spindle reverse jog phase shift， valid when the valid level is high
196-Enable the servo and enable the cam
197-Switching between fixed length or tracking
198-Clear wheel cutting alarm
199-The point cut is confirmed， the rising edge is valid
200-Order toggle switch 1， valid when the active level is high
201-Order toggle switch 2， valid when the active level is high
202-Positive phase shift of the spindle， trigger once， the spindle increases the displacement of P15.61， the rising edge is valid
203-Negative phase shift of the spindle， trigger once， the spindle reduces the displacement of P15.61， the rising edge is valid
204-Increase the cutting length of the current order， trigger once， the current order increases the length of P15.37， the rising edge is valid
205-Decrease the cutting length of the current order， trigger once， the current order will reduce the length of P15.37， the rising edge is valid
206-Counter 1 clearing bit， clearing P15.52， valid when the effective level is high
207-Counter 2 clearing bit， clearing P15.57， valid when the effective level is high
208-Clear the lost label count P16.43， valid at the rising edge
209-Sampling length， the next cycle runs according to the immediate cutting length， the rising edge is valid
210-Cam emergency stop
211-In point cam mode， switch to auxiliary color scale. When in effect， a secondary color scale is used.
212-In point cam mode， auxiliary color scale.