Rate Current(A),125
Max Current Percent(%),200
Rate Speed(rpm),1000
Max Speed(rpm),1200
Rotor Innertia(kgcm2),1100
Rate Torque(NM),600
EMF(V/Krpm),315
Stator Register(om),0.094
Stator Induct(mL),3.131
Electric Time Constant(ms),33
Pair of Poles,4
Encoder Type,12
Encoder Pulses Per Round,16777216
AB phase,1
Z point offset,9295
HALL1 electric angle,425
HALL2 electric angle,85
HALL3 electric angle,255
HALL4 electric angle,765
HALL5 electric angle,595
HALL6 electric angle,935
Default current loop bandwidth,600
Default speed loop bandwidth,20
Default encoder filter ,10
Default encoder sample period setting ,0
Others Parameter Set:

