Rate Current(A),2.8
Max Current Percent(%),250
Rate Speed(rpm),3000
Max Speed(rpm),6000
Rotor Innertia(kgcm2),0.55
Rate Torque(NM),1.27
EMF(V/Krpm),0
Stator Register(om),3
Stator Induct(mL),9.48
Electric Time Constant(ms),3
Pair of Poles,4
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Z point offset,2486
HALL1 electric angle,441
HALL2 electric angle,92
HALL3 electric angle,265
HALL4 electric angle,776
HALL5 electric angle,608
HALL6 electric angle,944
Default current loop bandwidth,2035
Default speed loop bandwidth,13
Default encoder filter ,5,0
Default encoder sample period setting ,0
Others Parameter Set:

