Rate Current(A),89.7
Max Current Percent(%),200
Rotor Innertia(kgcm2),42000
Rate Torque(NM),438.5
Stator Register(om),0.5
Rotor Register(om),0.5
Total Leak Induct(mL),1.0
Lm Induct(mL),250
Rate Freq(Hz),50
Max Freq(Hz),300
Pair of Poles,3
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Default current loop bandwidth,500
Default speed loop bandwidth,15
Default encoder filter ,10
Default encoder sample period setting ,0
Others Parameter Set:

