Version,1
Rate Current(A),6.4
Max Current Percent(%),200
Rate Speed(rpm),3000
Max Speed(rpm),4600
Rotor Innertia(kgcm2),3.74
Rate Torque(NM),5
EMF(V/Krpm),60
Stator Register(om),0.81
Stator Induct(mL),2.59
Electric Time Constant(ms),3.2
Pair of Poles,4
Encoder Type,12
Encoder Pulses Per Round,16777216
AB phase,1
Z point offset,9177
HALL1 electric angle,425
HALL2 electric angle,85
HALL3 electric angle,255
HALL4 electric angle,765
HALL5 electric angle,595
HALL6 electric angle,935
Default current loop bandwidth,1000
Default speed loop bandwidth,20
Default encoder filter ,5,0.1
Default encoder sample period setting ,4
BissC MultiTurn Bit length ,12
BissC SingleTurn Bit length ,24
BissC Status Bit length ,2
BissC Normal Status Value ,3
BissC ACK time ,50
BissC Timeout  ,50
Others Parameter Set:

