Rate Current(A),6
Max Current Percent(%),300
Rate Speed(rpm),2500
Max Speed(rpm),3000
Rotor Innertia(kgcm2),10
Rate Torque(NM),6
EMF(V/Krpm),0
Stator Register(om),3.38
Stator Induct(mL),8.72
Electric Time Constant(ms),2
Pair of Poles,4
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Z point offset,2459
HALL1 electric angle,446
HALL2 electric angle,106
HALL3 electric angle,277
HALL4 electric angle,784
HALL5 electric angle,611
HALL6 electric angle,957
Default current loop bandwidth,2035
Default speed loop bandwidth,25
Default encoder filter ,5,0
Default encoder sample period setting ,0
Others Parameter Set:

