Rate Current(A),3
Max Current Percent(%),250
Rate Speed(rpm),3000
Max Speed(rpm),4500
Rotor Innertia(kgcm2),2
Rate Torque(NM),2.39
EMF(V/Krpm),0
Stator Register(om),3.7
Stator Induct(mL),5.68
Electric Time Constant(ms),1
Pair of Poles,4
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Z point offset,2416
HALL1 electric angle,457
HALL2 electric angle,104
HALL3 electric angle,269
HALL4 electric angle,793
HALL5 electric angle,627
HALL6 electric angle,960
Default current loop bandwidth,1850
Default speed loop bandwidth,25
Default encoder filter ,5,0
Default encoder sample period setting ,0
Others Parameter Set:

