47-Tension compensation direction (order switch 1) 
48-Tracking direction (order toggle switch 2) 
49-Force clipping at maximum compensation speed (spindle point-to-point positive phase shift) 
50-Prohibit winding diameter calculation (spindle point-to-point negative phase shift) 
51-Roll change (increase cut length) 
52-Initial coil diameter switch (reduce cutting length) 
53-Clear feed length (counter 1 clear bit) 
54-Forced fast tightening (counter 2 clear bit) 
55-Disable tension compensation in closed-loop speed mode 
65-SPEED MODE UPDOWN MODE HOLD SIGNAL 
66-Return to the previous phase (tension type: enable velocity stacking) 
68-Go to the specified phase (tension type: Closed-loop speed torque mode IO switching)(point cam color code switching) 
69-Fixed position for forward jog (tension type: Motor rotation direction in closed-loop speed mode)(second color code of point cam) 
70-Reverse jog fixed position (tension version: Motor rotation direction in closed-loop torque mode)(tangent point confirmation DI)
71- The gantry synchronization position error is cleared, and it is valid when the effective level is high
72 - Synchronization enable, valid when the active level is high
73-CAM pause signal， effective when the effective level is high.
74 - Origin return to zero, rising edge is valid
75-Host origin signal, connected to the host, fixed drive DI9
76-Slave origin signal, connected to the slave, fixed driver DI10
77-Colour mark manual shielding input， effective when the effective level is high， colour mark trigger is invalid when effective
78-Feeding detection signal， effective when the effective level is high
79-Cut the signal immediately， the rising edge is valid
80-Trigger an interrupt event， the rising edge is valid
81-Switch from the interrupt event to the cam mode， the cam re-engages， and the rising edge is valid
82-Clear the number of effective switching points P16.07， effective when the effective level is high
83-Clear the total number of cuts P16.08， order 1 count P15.91， order 2 count P15.92， order 3 count P15.93， order 4 count P15.94， valid when the effective level is high
84-Clear the colour mark count P16.35， valid when the effective level is high
85-The current order count is cleared， valid when the effective level is high
86-The wheel tangent is jog in the positive direction， it can only be used when it is disengaged， and it is effective when the effective level is high.
87-The wheel tangent is jog in the reverse direction， it can only be used when it is disengaged， and it is effective when the effective level is high.
88-Spindle positive jog phase shift， effective when the effective level is high
89-Spindle reverse jog phase shift， effective when the effective level is high
90-pull gauge signal 
91-single signal 
92-double sheet signal 
93-Increase the distance from the pull gauge to the tangent point 
94-Reduce the distance from the pull gauge to the tangent point 
95-Relearn the distance from the pull gauge to the tangent point