Version,2
Rate Current(A),4.6
Max Current Percent(%),300
Rate Speed(mm/s),1000
Max Speed(mm/s),2000
Mover mass(kg),3.01
Rate Force(N),330.4
EMF(Vrms/m/s),0
Stator Register(om),2.18
Stator Induct(mL),7.18
Electric Time Constant(ms),6
Magnetic pole pitch(mm),20
Encoder resolution (um),1
res1,0 
res2,0
Encoder Type,9
AB phase,0
Z point offset,0
HALL1 electric angle,425
HALL2 electric angle,85
HALL3 electric angle,255
HALL4 electric angle,765
HALL5 electric angle,595
HALL6 electric angle,935
Default current loop bandwidth,1035
Default speed loop bandwidth,10
Default encoder filter ,5,0
Default encoder sample period setting ,0
BissC MultiTurn Bit length ,12
BissC SingleTurn Bit length ,24
BissC Status Bit length ,2
BissC Normal Status Value ,3
BissC ACK time ,5
BissC Timeout  ,50
Default postion loop bandwidth,30
Default Load Inertia Ratio,3.0
res3,0 
res4,0
res5,0
Others Parameter Set:

