80-Copier Mode
81-External emergency stop input，valid when the valid level is high
82-Trigger stamping，the rising edge of the signal is valid
83-Trigger the handle，the rising edge is valid
84-Jog down，The rising edge of the signal is valid
85-Jog up，The rising edge of the signal is valid