Rate Current(A),15.5
Max Current Percent(%),300
Rate Speed(rpm),1500
Max Speed(rpm),3000
Rotor Innertia(kgcm2),76.6
Rate Torque(NM),28.4
EMF(V/Krpm),0
Stator Register(om),0.98
Stator Induct(mL),9.42
Electric Time Constant(ms),9
Pair of Poles,5
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Z point offset,1999
HALL1 electric angle,439
HALL2 electric angle,83
HALL3 electric angle,255
HALL4 electric angle,772
HALL5 electric angle,605
HALL6 electric angle,938
Default current loop bandwidth,2035
Default speed loop bandwidth,15
Default encoder filter ,5,0
Default encoder sample period setting ,0
Others Parameter Set:

