Rate Current(A),5
Max Current Percent(%),250
Rate Speed(rpm),1500
Max Speed(rpm),1800
Rotor Innertia(kgcm2),35.27
Rate Torque(NM),15
EMF(V/Krpm),0
Stator Register(om),5.22
Stator Induct(mL),14.5
Electric Time Constant(ms),2
Pair of Poles,4
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Z point offset,2437
HALL1 electric angle,454
HALL2 electric angle,99
HALL3 electric angle,267
HALL4 electric angle,791
HALL5 electric angle,624
HALL6 electric angle,957
Default current loop bandwidth,2035
Default speed loop bandwidth,13
Default encoder filter ,5,0
Default encoder sample period setting ,0
Others Parameter Set:

