Rate Current(A),22.1
Max Current Percent(%),150
Rotor Innertia(kgcm2),510
Rate Torque(NM),105
Stator Register(om),0.8
Rotor Register(om),0.6
Total Leak Induct(mL),3.5
Lm Induct(mL),150
Rate Freq(Hz),33.3
Max Freq(Hz),133.2
Pair of Poles,2
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Default current loop bandwidth,1000
Default speed loop bandwidth,50
Default encoder filter ,5
Default encoder sample period setting ,2
Others Parameter Set:
