620-The origin is not reset-solution: 1_reset before engagement 
621-Cam cycle error-solution: 1_overshear parameter setting is unreasonable, 2_feeding speed is too fast, 3_cutting material is too short 
622-Cam reversal-solution: 1_2nd encoder direction is negative, 2_XY pulse direction is negative