Rate Current(A),36.3
Max Current Percent(%),200,38.2
Rotor Innertia(kgcm2),2550
Rate Torque(NM),177
Stator Register(om),0.26
Rotor Register(om),0.4
Total Leak Induct(mL),3.8
Lm Induct(mL),72
Rate Freq(Hz),30
Max Freq(Hz),133.2
Pair of Poles,2
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Default current loop bandwidth,1000
Default speed loop bandwidth,20
Default encoder filter ,5
Default encoder sample period setting ,2
Others Parameter Set:

