47-(Spindle speed control enable bit) Tension compensation direction (order switch 1) 
48-(rigid tapping spindle speed control enable bit) tracking direction (order switch 2) 
49-(stop allowed) limit at the maximum compensation speed (spindle point-to-point positive phase shift) 
50-(the second stop) prohibit the calculation of winding diameter (spindle point-to-point negative phase shift) 
51-(Proximity switch) Roll change (increase cutting length) 
52-(Swing) Initial roll diameter switch (reduce cutting length) 
53-Clear feed length (counter 1 clear bit) 
54-Forced fast tightening (counter 2 clear bit) 
55-Disable tension compensation in closed-loop speed mode 
65-SPEED MODE UPDOWN MODE HOLD SIGNAL 
66-Return to the previous phase (tension type: enable velocity stacking) 
68-Go to the specified phase (tension type: Closed-loop speed torque mode IO switching) 
69-Fixed position for forward jog (tension type: Motor rotation direction in closed loop speed mode) 
70-Reverse jog fixed position (tension version: Motor rotation direction in closed-loop torque mode)(tangent point confirmation DI)
71-switch between XY pulse of cam spindle position source and that second encoder 
72-Cam Enable 
73-Pause cam input 
74-Wheel switching back to zero input bit 
75-Round cut Mark color code signal input 
76-Wheel cutting origin signal input 
77-Color-coded DI mask 
78-Feeding detection position 
79-Immediate cut signal input 
80-Trigger interrupt event 
81-Switch from interrupt event to cam mode 
82-Clear Cut Count 
83-Zero the total number of cuts 
84-Color mark counting zero clearing 
85-Current Order Count Zero 
86-Forward inching of wheel cutting slave shaft 
87-Inching in reverse direction of wheel cutting driven shaft 
88-positive inching phase-shifting of wheel cutting spindle 
89-Reverse inching phase shift of wheel cutting spindle 
90-pull gauge signal 
91-single signal 
92-double sheet signal 
93-Increase the distance from the pull gauge to the tangent point 
94-Reduce the distance from the pull gauge to the tangent point 
95-Relearn the distance from the pull gauge to the tangent point
