Rate Current(A),3.39
Max Current Percent(%),305
Rate Speed(mm/s),1000
Max Speed(mm/s),3000
Mover mass(kg),1.74
Rate Force(N),83
EMF(Vrms/m/s),0
Stator Register(om),3.66
Stator Induct(mL),7.16
Electric Time Constant(ms),3
Magnetic pole pitch(mm),25
Encoder resolution (um),2.5
res1,0 
res2,0
Encoder Type,9
AB phase,1
Z point offset,0
HALL1 electric angle,425
HALL2 electric angle,85
HALL3 electric angle,255
HALL4 electric angle,765
HALL5 electric angle,595
HALL6 electric angle,935
Default current loop bandwidth,1050
Default speed loop bandwidth,20
Default encoder filter ,5,0
Default encoder sample period setting ,0
res3,0 
res4,0
Others Parameter Set:

