40-Output in meshing state, output valid signal when meshing
41-The output is valid when the slave axis is in the synchronization zone
42-The order is close to the output
43-order completion output
44-The number of color mark loss reached
45-Counter 1 reaches the output
46-Counter 2 reaches the output
47-Output angle range 1 of slave axis
48-Output angle range 2 of slave axis
49-Output angle range 3 of slave axis
50-Output angle range 4 of slave axis
51-Color mark trigger valid range output
52-Output signal the colour mark trace success
53-Curve running output
54-Cam curve segment output of 1
55-Cam curve segment output of 2
56-Automatically correct the tangent point output
57-Point Cam allows first color mark triggering
58-Point Cam allows secondary color mark triggering
59-Point Cam Alarm
60-Point cam speed is too fast