Rate Current(A),2.5
Max Current Percent(%),300
Rate Speed(rpm),3000
Max Speed(rpm),6000
Rotor Innertia(kgcm2),0.44
Rate Torque(NM),1.27
EMF(V/Krpm),30
Stator Register(om),2.6
Stator Induct(mL),5.8
Electric Time Constant(ms),2.2
Pair of Poles,5
Encoder Type,6
Encoder Pulses Per Round,8388608
AB phase,0
Z point offset,0
HALL1 electric angle,425
HALL2 electric angle,85
HALL3 electric angle,255
HALL4 electric angle,765
HALL5 electric angle,595
HALL6 electric angle,935
Default current loop bandwidth,800
Default speed loop bandwidth,30
Default encoder filter ,5
Default encoder sample period setting ,5
Others Parameter Set:

