Rate Current(A),4.2
Max Current Percent(%),350
Rate Speed(rpm),3000
Max Speed(rpm),5000
Rotor Innertia(kgcm2),1.71
Rate Torque(NM),2.39
EMF(V/Krpm),36.6
Stator Register(om),1.65
Stator Induct(mL),7.4
Electric Time Constant(ms),4.48
Pair of Poles,5
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,1
Z point offset,124
HALL1 electric angle,538
HALL2 electric angle,873
HALL3 electric angle,703
HALL4 electric angle,191
HALL5 electric angle,407
HALL6 electric angle,20
Default current loop bandwidth,1000
Default speed loop bandwidth,50
Default encoder filter ,5
Default encoder sample period setting ,5
Others Parameter Set:

