Rate Current(A),9.5
Max Current Percent(%),200
Rate Speed(rpm),1500
Max Speed(rpm),1800
Rotor Innertia(kgcm2),27.7
Rate Torque(NM),15
EMF(V/Krpm),114
Stator Register(om),1.1
Stator Induct(mL),4.45
Electric Time Constant(ms),4.05
Pair of Poles,4
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,1
Z point offset,120
HALL1 electric angle,545
HALL2 electric angle,885
HALL3 electric angle,715
HALL4 electric angle,203
HALL5 electric angle,409
HALL6 electric angle,30
Default current loop bandwidth,1000
Default speed loop bandwidth,50
Default encoder filter ,5
Default encoder sample period setting ,5
Others Parameter Set:

