Rate Current(A),56.5
Max Current Percent(%),200
Rotor Innertia(kgcm2),4400
Rate Torque(NM),191
Stator Register(om),1
Rotor Register(om),1
Total Leak Induct(mL),0.5
Lm Induct(mL),250
Rate Freq(Hz),50
Max Freq(Hz),200
Pair of Poles,2
Encoder Type,0
Encoder Pulses Per Round,10000
AB phase,0
Default current loop bandwidth,800
Default speed loop bandwidth,20
Default encoder filter ,5
Default encoder sample period setting ,0
Others Parameter Set:

